;
; Copyright 2012, Broadcom Corporation.
; All Rights Reserved.
;

[version]
Signature       = "$Windows NT$"                ; Combined WinXP/Vista inf
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %V_BCM%

DriverVer=07/08/2015, 1.455.0.0
CatalogFile     = bcmdhd63.cat

[Manufacturer]
        %V_BCM% = BROADCOM, NTamd64.6.2, NTx86.6.2

[ControlFlags]
        ExcludeFromSelect = *

[BROADCOM.NTamd64.6.2]
		%BCM435SD_DeviceDesc% = BCM435XNGSD_NT62, SD\VID_02D0&PID_4356&FN_1
		%BCM4343SD_DeviceDesc% = BCM4343XNGSD_NT62, SD\VID_02D0&PID_A9A6&FN_1

[BROADCOM.NTx86.6.2]
		%BCM435SD_DeviceDesc% = BCM435XNGSD_NT62, SD\VID_02D0&PID_4356&FN_1
		%BCM4343SD_DeviceDesc% = BCM4343XNGSD_NT62, SD\VID_02D0&PID_A9A6&FN_1

[BCM435XNGSD_NT62.NTamd64]
        Include         = netvwifibus.inf
        Needs           = VWiFiBus.CopyFiles
        *IfType         = 71    ; IF_TYPE_IEEE80211
        *MediaType      = 16    ; NdisMediumNative802_11
        *PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
        Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
        BusType         = 15    ; PNP bus
        AddReg          = BCM43XX_NT61.reg, BCMSDH43XX.brcm.reg, common.reg, common.vista.reg, gn.options.reg, bagn40.options.reg, nbg20.channels.reg, nbg40.channels.reg, wowl.std_keywords.reg, wowl.capabilities.enabled.reg
        CopyFiles       = BCM43XNXSD_NT60.files.NTamd64

[BCM435XNGSD_NT62.NTamd64.Services]
        Include = netvwifibus.inf
        Needs   = VWiFiBus.Services
        AddService = BCMSDH43XX, 2, BCMSDH43XX_NT60.Service.NTamd64, common.EventLog

[BCM435XNGSD_NT62.NTamd64.HW]
        Include = netvwifibus.inf
        Needs   = VWiFiBus.PnPFilterRegistration

[BCM4343XNGSD_NT62.NTamd64]
        Include         = netvwifibus.inf
        Needs           = VWiFiBus.CopyFiles
        *IfType         = 71    ; IF_TYPE_IEEE80211
        *MediaType      = 16    ; NdisMediumNative802_11
        *PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
        Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
        BusType         = 15    ; PNP bus
        AddReg          = BCM43XX_NT61.reg, BCMSDH43XX.brcm.reg, common.reg, common.vista.reg, gn.options.reg, nbg20.channels.reg, wowl.std_keywords.reg, wowl.capabilities.enabled.reg, BCMSDH4343.brcm.reg
        CopyFiles       = BCM4343XSD_NT60.files.NTamd64

[BCM4343XNGSD_NT62.NTamd64.Services]
        Include = netvwifibus.inf
        Needs   = VWiFiBus.Services
        AddService = BCMSDH43XX, 2, BCMSDH43XX_NT60.Service.NTamd64, common.EventLog

[BCM4343XNGSD_NT62.NTamd64.HW]
        Include = netvwifibus.inf
        Needs   = VWiFiBus.PnPFilterRegistration

[BCM435XNGSD_NT62.NTx86]
        Include         = netvwifibus.inf
        Needs           = VWiFiBus.CopyFiles
        *IfType         = 71    ; IF_TYPE_IEEE80211
        *MediaType      = 16    ; NdisMediumNative802_11
        *PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
        Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
        BusType         = 15    ; PNP bus
        AddReg          = BCM43XX_NT61.reg, BCMSDH43XX.brcm.reg, common.reg, common.vista.reg, gn.options.reg, bagn40.options.reg, nbg20.channels.reg, nbg40.channels.reg, wowl.std_keywords.reg, wowl.capabilities.enabled.reg
        CopyFiles       = BCM43XNXSD_NT60.files.NTx86

[BCM435XNGSD_NT62.NTx86.Services]
        Include = netvwifibus.inf
        Needs   = VWiFiBus.Services
        AddService = BCMSDH43XX, 2, BCMSDH43XX_NT60.Service.NTx86, common.EventLog

[BCM435XNGSD_NT62.NTx86.HW]
        Include = netvwifibus.inf
        Needs   = VWiFiBus.PnPFilterRegistration


[BCM4343XNGSD_NT62.NTx86]
        Include         = netvwifibus.inf
        Needs           = VWiFiBus.CopyFiles
        *IfType         = 71    ; IF_TYPE_IEEE80211
        *MediaType      = 16    ; NdisMediumNative802_11
        *PhysicalMediaType = 9  ; NdisPhysicalMediumNative802_11
        Characteristics = 0x84  ; NCF_PHYSICAL | NCF_HAS_UI
        BusType         = 15    ; PNP bus
        AddReg          = BCM43XX_NT61.reg, BCMSDH43XX.brcm.reg, common.reg, common.vista.reg, gn.options.reg, nbg20.channels.reg, wowl.std_keywords.reg, wowl.capabilities.enabled.reg, BCMSDH4343.brcm.reg
        CopyFiles       = BCM4343XSD_NT60.files.NTx86

[BCM4343XNGSD_NT62.NTx86.Services]
        Include = netvwifibus.inf
        Needs   = VWiFiBus.Services
        AddService = BCMSDH43XX, 2, BCMSDH43XX_NT60.Service.NTx86, common.EventLog

[BCM4343XNGSD_NT62.NTx86.HW]
        Include = netvwifibus.inf
        Needs   = VWiFiBus.PnPFilterRegistration

[BCM43XX_NT61.reg]
        ; Ndis Info
        ; Interfaces
        HKR,    Ndi\Interfaces, UpperRange,     ,       "ndis5"
        HKR,    Ndi\Interfaces, LowerRange,     ,       "ethernet,wlan,vwifi"

[BCMSDH43XX.brcm.reg]
        HKR,    Ndi,    HelpText,               ,       %BCM43XX_HELP%
        HKR,    Ndi,    Service,                0,      "BCMSDH43XX"

        HKR,     ,"featureflag",      65537, "0x00000004"

[BCMSDH4343.brcm.reg]
        HKR,    ,       "DongleConsoleMs",      0,      "0"

[common.EventLog]
        AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
        HKR,    ,       EventMessageFile,       0x00020000,     "%%SystemRoot%%\System32\netevent.dll"
        HKR,    ,       TypesSupported,         0x00010001,     7

[BCMSDH43XX_NT60.Service.NTamd64]
        DisplayName     = %BCMSDH43XX_Service_DispName%
        ServiceType     = 1                     ; %SERVICE_KERNEL_DRIVER%
        StartType       = 3                     ; %SERVICE_DEMAND_START%
        ErrorControl    = 1                     ; %SERVICE_ERROR_NORMAL%
        ServiceBinary   = %12%\bcmdhd63.sys
        LoadOrderGroup  = NDIS

[BCM43XNXSD_NT60.files.NTamd64]
        bcmdhd63.sys,,,6
        4356r2rtecdc.bin,4356a2rtecdc.bin,,6
        4356r2nvram.txt,bcm94356z_p122.txt,,6

; 11 == %windir%/system32
; 12 == %windir%/system32/drivers

[BCM4343XSD_NT60.files.NTamd64]
        bcmdhd63.sys,,,6
        43430r0rtecdc.bin,43438a0rtecdc.bin,,6
        43430r1rtecdc.bin,43438a1rtecdc.bin,,6
        43430r0nvram.txt,bcm943430wlselgs.txt,,6
        43430r1nvram.txt,bcm943430a1wlselgs.txt,,6

; 11 == %windir%/system32
; 12 == %windir%/system32/drivers


[BCMSDH43XX_NT60.Service.NTx86]
        DisplayName     = %BCMSDH43XX_Service_DispName%
        ServiceType     = 1                     ; %SERVICE_KERNEL_DRIVER%
        StartType       = 3                     ; %SERVICE_DEMAND_START%
        ErrorControl    = 1                     ; %SERVICE_ERROR_NORMAL%
        ServiceBinary   = %12%\bcmdhd63.sys
        LoadOrderGroup  = NDIS

[BCM43XNXSD_NT60.files.NTx86]
        bcmdhd63.sys,,,6
        4356r2rtecdc.bin,4356a2rtecdc.bin,,6
        4356r2nvram.txt,bcm94356z_p122.txt,,6

; 11 == %windir%/system32
; 12 == %windir%/system32/drivers

[BCM4343XSD_NT60.files.NTx86]
        bcmdhd63.sys,,,6
        43430r0rtecdc.bin,43438a0rtecdc.bin,,6
        43430r1rtecdc.bin,43438a1rtecdc.bin,,6
        43430r0nvram.txt,bcm943430wlselgs.txt,,6
        43430r1nvram.txt,bcm943430a1wlselgs.txt,,6

; 11 == %windir%/system32
; 12 == %windir%/system32/drivers




[DestinationDirs]
	DefaultDestDir                                = 11
	BCM43XNXSD_NT60.files.NTamd64                 = 12
	BCM43XNXSD_NT60.files.NTx86                   = 12
	BCM4343XSD_NT60.files.NTamd64                 = 12
	BCM4343XSD_NT60.files.NTx86                   = 12

[SourceDisksNames]
        1=%BCM43XX_DiskName%,,

; for WinVista specify bcmdhd63.sys
[SourceDisksFiles.amd64]
	bcmdhd63.sys=1
	;43241b4rtecdc.bin=1
	4356a2rtecdc.bin=1
	bcm94356z_p122.txt=1
	43438a0rtecdc.bin=1
	43438a1rtecdc.bin=1
	bcm943430wlselgs.txt=1
	bcm943430a1wlselgs.txt=1

[SourceDisksFiles.x86]
	bcmdhd63.sys=1
	;43241b4rtecdc.bin=1
	4356a2rtecdc.bin=1
	bcm94356z_p122.txt=1
	43438a0rtecdc.bin=1
	43438a1rtecdc.bin=1
	bcm943430wlselgs.txt=1
	bcm943430a1wlselgs.txt=1

;Uninstall
[Cleanup]

; common for WinVista, but excluded in WinXP and older
[common.vista.reg]
        HKR,    Ndi\params\*PriorityVLANTag, ParamDesc, 0,      %PriorityVLANTag%
        HKR,    Ndi\params\*PriorityVLANTag, type,      0,      "enum"
        HKR,    Ndi\params\*PriorityVLANTag\enum, "0",  0,      %PriorityAndVLANDisabled%
        HKR,    Ndi\params\*PriorityVLANTag\enum, "1",  0,      %PriorityEnabled%
        HKR,    Ndi\params\*PriorityVLANTag\enum, "2",  0,      %VLANEnabled%
        HKR,    Ndi\params\*PriorityVLANTag\enum, "3",  0,      %PriorityAndVLANEnabled%
        HKR,    Ndi\params\*PriorityVLANTag,default,,"0"
        HKR,    Ndi\params\*PriorityVLANTag,optional,,"0"

; common for all platform
[common.reg]
;        HKR,    ,"DongleImagePath",       0,      "\SystemRoot\system32\drivers\rtecdc.bin"
;        HKR,    ,"SROMImagePath",         0,      "\SystemRoot\system32\drivers\nvram.txt"
        HKLM,system\CurrentControlSet\Services\NativeWiFiP\Parameters,EnableWoWLAN,0x00010001,1

        HKR,    Ndi\Params\*PacketCoalescing,  ParamDesc,  0, "Packet Coalescing"
        HKR,    Ndi\Params\*PacketCoalescing,  Type,       0, "enum"
        HKR,    Ndi\Params\*PacketCoalescing,  Default,    0, "1"
        HKR,    Ndi\Params\*PacketCoalescing\enum,   "0",  0, "Disabled"
        HKR,    Ndi\Params\*PacketCoalescing\enum,   "1",  0, "Enabled"

        HKR, Ndi\Params\*WakeOnPattern,  ParamDesc,  0, "Wake on pattern match"
        HKR, Ndi\Params\*WakeOnPattern,  Type,       0, "enum"
        HKR, Ndi\Params\*WakeOnPattern,  Default,    0, "1"
        HKR, Ndi\Params\*WakeOnPattern\enum,   "0",  0, "Disabled"
        HKR, Ndi\Params\*WakeOnPattern\enum,   "1",  0, "Enabled"

        HKR, Ndi\Params\*PMWiFiRekeyOffload,  ParamDesc,  0, "Wake on RSN Rekey"
        HKR, Ndi\Params\*PMWiFiRekeyOffload,  Type,       0, "enum"
        HKR, Ndi\Params\*PMWiFiRekeyOffload,  Default,    0, "1"
        HKR, Ndi\Params\*PMWiFiRekeyOffload\enum,   "0",  0, "Disabled"
        HKR, Ndi\Params\*PMWiFiRekeyOffload\enum,   "1",  0, "Enabled"

        HKR,    Ndi\params\RoamDelta, ParamDesc,        0,      %RoamingTendency%
        HKR,    Ndi\params\RoamDelta, type,             0,      "enum"
        HKR,    Ndi\params\RoamDelta\enum, "0",         0,      %Aggressive%
        HKR,    Ndi\params\RoamDelta\enum, "1",         0,      %Moderate%
        HKR,    Ndi\params\RoamDelta\enum, "2",         0,      %Conservative%
        HKR,    Ndi\params\RoamDelta\enum, "3",         0,      %Auto%
        HKR,    Ndi\params\RoamDelta,default,,"3"

        HKR,    Ndi\params\MPC, ParamDesc,              0,      %MinimumPowerConsumption%
        HKR,    Ndi\params\MPC, type,                   0,      "enum"
        HKR,    Ndi\params\MPC\enum, "0",               0,      %Disabled%
        HKR,    Ndi\params\MPC\enum, "1",               0,      %Enabled%
        HKR,    Ndi\params\MPC,default,,"1"

        HKR,    Ndi\params\frag, ParamDesc,     0,      %FragmentationThreshold%
        HKR,    Ndi\params\frag,type,0,"dword"
        HKR,    Ndi\params\frag,min,,"256"
        HKR,    Ndi\params\frag,max,,"2346"
        HKR,    Ndi\params\frag,default,,"2346"

        HKR,    Ndi\params\rts, ParamDesc,      0,      %RTSThreshold%
        HKR,    Ndi\params\rts,type,0,"dword"
        HKR,    Ndi\params\rts,min,,"0"
        HKR,    Ndi\params\rts,max,,"2347"
        HKR,    Ndi\params\rts,default,,"2347"

        HKR,    Ndi\params\NetworkAddress, ParamDesc,   0, %LocallyAdministeredMACAddress%
        HKR,    Ndi\params\NetworkAddress, type,        0, "edit"
        HKR,    Ndi\params\NetworkAddress, LimitText,   0, "12"
        HKR,    Ndi\params\NetworkAddress, UpperCase,  0, "1"
        HKR,    Ndi\params\NetworkAddress, default,     0, ""
        HKR,    Ndi\params\NetworkAddress, optional,    0, "1"

        HKR,    Ndi\params\PwrOut, ParamDesc,   0,      %PowerOutput%
        HKR,    Ndi\params\PwrOut, type,                0,      "enum"
        HKR,    Ndi\params\PwrOut\enum, "100",  0,      "100%%"
        HKR,    Ndi\params\PwrOut\enum, "75",   0,      "75%%"
        HKR,    Ndi\params\PwrOut\enum, "50",   0,      "50%%"
        HKR,    Ndi\params\PwrOut\enum, "25",   0,      "25%%"
        HKR,    Ndi\params\PwrOut,default,,"100"

        HKR,    Ndi\params\FrameBursting, ParamDesc,    0,      %XPress_Technology%
        HKR,    Ndi\params\FrameBursting, type,         0,      "enum"
        HKR,    Ndi\params\FrameBursting\enum, "0",             0,      %Disabled%
        HKR,    Ndi\params\FrameBursting\enum, "1",             0,      %Enabled%
        HKR,    Ndi\params\FrameBursting,default,,"0"

        HKR,    Ndi\params\BTCoexist, ParamDesc,        0,      %BlueToothCollaboration%
        HKR,    Ndi\params\BTCoexist, type,             0,      "enum"
        HKR,    Ndi\params\BTCoexist\enum, "0", 0,      %Disable%
        HKR,    Ndi\params\BTCoexist\enum, "1", 0,      %Enable%
        HKR,    Ndi\params\BTCoexist\enum, "3", 0,      %Auto%
        HKR,    Ndi\params\BTCoexist,default,,"3"

        HKR,    Ndi\params\WakeUpCapabilities, ParamDesc,       0,      %WakeUpCapabilities%
        HKR,    Ndi\params\WakeUpCapabilities, type,            0,      "enum"
        HKR,    Ndi\params\WakeUpCapabilities\enum, "0",        0,      %None%
        HKR,    Ndi\params\WakeUpCapabilities\enum, "2",        0,      %NetPattern%
        HKR,    Ndi\params\WakeUpCapabilities\enum, "28",       0,      %LossofAP%
        HKR,    Ndi\params\WakeUpCapabilities\enum, "30",       0,      %LossNet%
        HKR,    Ndi\params\WakeUpCapabilities\enum, "31",       0,      %All%
        HKR,    Ndi\params\WakeUpCapabilities,default,,"3"

        HKR,    Ndi\params\antdiv, ParamDesc,   0,      %AntennaDiversity%
        HKR,    Ndi\params\antdiv, type,        0,      "enum"
        HKR,    Ndi\params\antdiv\enum, "-1",   0,      %Auto%
        HKR,    Ndi\params\antdiv\enum, "0",    0,      %Main%
        HKR,    Ndi\params\antdiv\enum, "1",    0,      %Aux%
        HKR,    Ndi\params\antdiv,default,,"-1"

        HKR,    Ndi\params\WME, ParamDesc,      0,      %WME%
        HKR,    Ndi\params\WME, type,           0,      "enum"
        HKR,    Ndi\params\WME\enum, "-1",      0,      %Auto%
        HKR,    Ndi\params\WME\enum, "1",       0,      %Enabled%
        HKR,    Ndi\params\WME\enum, "0",       0,      %Disabled%
        HKR,    Ndi\params\WME,default,,"-1"

        HKR,    Ndi\params\BtAmp, ParamDesc,    0,      %BTAMP%
        HKR,    Ndi\params\BtAmp, type,         0,      "enum"
        HKR,    Ndi\params\BtAmp\enum, "0",     0,      %Disabled%
        HKR,    Ndi\params\BtAmp\enum, "1",     0,      %Enabled%
        HKR,    Ndi\params\BtAmp,default,,"1"

        HKR,    Ndi\params\ListenInterval, ParamDesc,     0,      %ListenInterval%
        HKR,    Ndi\params\ListenInterval,type,0,"dword"
        HKR,    Ndi\params\ListenInterval,min,,"1"
        HKR,    Ndi\params\ListenInterval,max,,"100"
        HKR,    Ndi\params\ListenInterval,default,,"1"

        HKR,    Ndi\params\D2ListenInterval, ParamDesc,     0,      %D2ListenInterval%
        HKR,    Ndi\params\D2ListenInterval,type,0,"dword"
        HKR,    Ndi\params\D2ListenInterval,min,,"1"
        HKR,    Ndi\params\D2ListenInterval,max,,"100"
        HKR,    Ndi\params\D2ListenInterval,default,,"5"

        HKR,    Ndi\params\WFDChannelNumber, ParamDesc,     0,      %WFDChannelNumber%
        HKR,    Ndi\params\WFDChannelNumber,type,0,"dword"
        HKR,    Ndi\params\WFDChannelNumber,min,,"1"
        HKR,    Ndi\params\WFDChannelNumber,max,,"11"
        HKR,    Ndi\params\WFDChannelNumber,default,,"11"

        HKR,    Ndi\params\EnableLTR, ParamDesc,0, %EnableLTR%
        HKR,    Ndi\params\EnableLTR, type,     0,         "enum"
        HKR,    Ndi\params\EnableLTR\enum, "0", 0, %Disabled%
        HKR,    Ndi\params\EnableLTR\enum, "1", 0, %Enabled%
        HKR,    Ndi\params\EnableLTR,default,,"1"

        HKR,    Ndi\params\LTR_ActiveValue, ParamDesc,     0,      %LTR_ActiveValue%
        HKR,    Ndi\params\LTR_ActiveValue,type,0,"dword"
        HKR,    Ndi\params\LTR_ActiveValue,min,,"0"
        HKR,    Ndi\params\LTR_ActiveValue,max,,"1023"
        HKR,    Ndi\params\LTR_ActiveValue,default,,"60"

        HKR,                                    ,"mchan_algo_wfd",                0,      "1"
        HKR,                                    ,"mchan_bw_wfd",                0,      "40"

[nbg20.channels.reg]
        ; Chanspec parameters
        ; 2G-band, 20MHz channels supported
        HKR,    Ndi\params\Chanspec\enum, "1",   0, "  1(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "2",   0, "  2(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "3",   0, "  3(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "4",   0, "  4(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "5",   0, "  5(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "6",   0, "  6(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "7",   0, "  7(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "8",   0, "  8(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "9",   0, "  9(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "10",   0, " 10(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "11",   0, " 11(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "12",   0, " 12(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "13",   0, " 13(20MHz)"
        HKR,    Ndi\params\Chanspec\enum, "14",   0, " 14(20MHz)"

[nbg40.channels.reg]
        ; 2G-band, 40MHz channels supported
        HKR,    Ndi\params\Chanspec\enum, "1bl",   0, "  1(40MHz-L)"
        HKR,    Ndi\params\Chanspec\enum, "6bl",   0, "  6(40MHz-L)"
        HKR,    Ndi\params\Chanspec\enum, "6bu",   0, "  6(40MHz-U)"
        HKR,    Ndi\params\Chanspec\enum, "11bu",  0, " 11(40MHz-U)"

[gn.options.reg]
        HKR,    Ndi\params\RoamTrigger, ParamDesc,      0,      %RoamingDecision%
        HKR,    Ndi\params\RoamTrigger, type,           0,      "enum"
        HKR,    Ndi\params\RoamTrigger\enum, "3",       0,      %Auto%
        HKR,    Ndi\params\RoamTrigger\enum, "1",       0,      %OptimizeBandwidth%
        HKR,    Ndi\params\RoamTrigger\enum, "0",       0,      %Default%
        HKR,    Ndi\params\RoamTrigger\enum, "2",       0,      %OptimizeDistance%
        HKR,    Ndi\params\RoamTrigger,default,,"3"

        HKR,    Ndi\params\PLCPHeader, ParamDesc,       0,      %BSSPLCPHeader%
        HKR,    Ndi\params\PLCPHeader, type,            0,      "enum"
        HKR,    Ndi\params\PLCPHeader\enum, "-1",       0,      %Long%
        HKR,    Ndi\params\PLCPHeader\enum, "0",        0,      %AutoShortLong%
        HKR,    Ndi\params\PLCPHeader,default,,"0"

        HKR,    Ndi\params\IBSSMode, ParamDesc, 0,      %IBSSMode%
        HKR,    Ndi\params\IBSSMode, type,         0,      "enum"
        HKR,    Ndi\params\IBSSMode\enum, "0",     0,      %80211bOnly%
        HKR,    Ndi\params\IBSSMode\enum, "2",     0,      %54gAuto%
        HKR,    Ndi\params\IBSSMode\enum, "4",     0,      %54gPerformance%
        HKR,    Ndi\params\IBSSMode\enum, "5",     0,      %80211bgnAuto%
        HKR,    Ndi\params\IBSSMode,default,,"0"

        HKR,    Ndi\params\IBSSGProtection, ParamDesc,  0,      %IBSS54gtmProtectionMode%
        HKR,    Ndi\params\IBSSGProtection, type,       0,      "enum"
        HKR,    Ndi\params\IBSSGProtection\enum, "0",   0,      %Disabled%
        HKR,    Ndi\params\IBSSGProtection\enum, "2",   0,      %Auto%
        HKR,    Ndi\params\IBSSGProtection,default,,"2"

        HKR,    Ndi\params\Intolerant, ParamDesc,       0,      %Intolerant%
        HKR,    Ndi\params\Intolerant, type,         0,      "enum"
        HKR,    Ndi\params\Intolerant\enum, "0",     0,      %Disabled%
        HKR,    Ndi\params\Intolerant\enum, "1",     0,      %Enabled%
        HKR,    Ndi\params\Intolerant,default,,"0"

        HKR,    Ndi\params\OBSSCoex, ParamDesc, 0,      %OBSSCoex%
        HKR,    Ndi\params\OBSSCoex, type,      0,      "enum"
        HKR,    Ndi\params\OBSSCoex\enum, "0",  0,      %Disabled%
        HKR,    Ndi\params\OBSSCoex\enum, "1",  0,      %Enabled%
        HKR,    Ndi\params\OBSSCoex\enum, "-1", 0,      %Auto%
        HKR,    Ndi\params\OBSSCoex,default,,"-1"

        ; option to override antenna selection, -1: no override, 0: no selection
        HKR,                                    ,"mimo_antsel", 0,      "-1"

; options for 40MHz band for n
[bagn40.options.reg]
        HKR,    Ndi\params\BandwidthCap, ParamDesc,     0,      "Bandwidth Capability"
        HKR,    Ndi\params\BandwidthCap, type,          0,      "enum"
        HKR,    Ndi\params\BandwidthCap\enum, "0",      0,      "11a/b/g:20MHz"
        HKR,    Ndi\params\BandwidthCap\enum, "1",      0,      "11a/b/g:20/40MHz"
        HKR,    Ndi\params\BandwidthCap\enum, "2",      0,      "11a:20/40;11bg:20MHz"
        HKR,    Ndi\params\BandwidthCap,default,,"2"

[wowl.capabilities.enabled.reg]
        HKR,,   "WakeUpCapabilities", 0x00010001, "0xffffffff"

[wowl.capabilities.disabled.reg]
        HKR,,   "WakeUpCapabilities", 0x00010001, "0x00000000"

[wowl.std_keywords.reg]
        HKR, Ndi\params\*WakeOnMagicPacket, ParamDesc,  0, %WakeOnMagicPacket%
        HKR, Ndi\params\*WakeOnMagicPacket, type,       0, "enum"
        HKR, Ndi\params\*WakeOnMagicPacket\enum,        "0", 0, %Disabled%
        HKR, Ndi\params\*WakeOnMagicPacket\enum,        "1", 0, %Enabled%
        HKR, Ndi\params\*WakeOnMagicPacket,default,,    "1"
        HKR, Ndi\params\*WakeOnMagicPacket,optional,,   "0"

        HKR, Ndi\params\*WakeOnPattern, ParamDesc,      0, %WakeOnPatternMatch%
        HKR, Ndi\params\*WakeOnPattern, type,           0, "enum"
        HKR, Ndi\params\*WakeOnPattern\enum,            "0", 0, %Disabled%
        HKR, Ndi\params\*WakeOnPattern\enum,            "1", 0, %Enabled%
        HKR, Ndi\params\*WakeOnPattern,default,,        "1"
        HKR, Ndi\params\*WakeOnPattern,optional,,       "0"

        HKR, Ndi\params\*PMARPOffload, ParamDesc,       0, %ARPOffload%
        HKR, Ndi\params\*PMARPOffload, type,            0, "enum"
        HKR, Ndi\params\*PMARPOffload\enum,             "0", 0, %Disabled%
        HKR, Ndi\params\*PMARPOffload\enum,             "1", 0, %Enabled%
        HKR, Ndi\params\*PMARPOffload,default,,         "1"
        HKR, Ndi\params\*PMARPOffload,optional,,        "0"

        HKR, Ndi\params\*PMNSOffload, ParamDesc,        0, %NSOffload%
        HKR, Ndi\params\*PMNSOffload, type,             0, "enum"
        HKR, Ndi\params\*PMNSOffload\enum,              "0", 0, %Disabled%
        HKR, Ndi\params\*PMNSOffload\enum,              "1", 0, %Enabled%
        HKR, Ndi\params\*PMNSOffload,default,,          "1"
        HKR, Ndi\params\*PMNSOffload,optional,,         "0"

        HKR, Ndi\params\*PMWiFiRekeyOffload, ParamDesc, 0, %WiFiRekeyingOffload%
        HKR, Ndi\params\*PMWiFiRekeyOffload, type,      0, "enum"
        HKR, Ndi\params\*PMWiFiRekeyOffload\enum,       "0", 0, %Disabled%
        HKR, Ndi\params\*PMWiFiRekeyOffload\enum,       "1", 0, %Enabled%
        HKR, Ndi\params\*PMWiFiRekeyOffload,default,,   "1"
        HKR, Ndi\params\*PMWiFiRekeyOffload,optional,,  "0"

[cs.std_keywords.reg]

	HKR,    Ndi\Params\*PacketCoalescing,  ParamDesc,  0, "Packet Coalescing"
	HKR,    Ndi\Params\*PacketCoalescing,  Type,       0, "enum"
	HKR,    Ndi\Params\*PacketCoalescing,  Default,    0, "1"
	HKR,    Ndi\Params\*PacketCoalescing\enum,   "0",  0, "Disabled"
	HKR,    Ndi\Params\*PacketCoalescing\enum,   "1",  0, "Enabled"

[strings]
V_BCM="Broadcom"
BCM43XX_HELP="The Broadcom 802.11 Network Adapter provides wireless local area networking."
BCM43XX_Service_DispName="Broadcom 802.11 Network Adapter Driver"
BCM43XX_DiskName="802.11 Network Adapter Install Disk"
BCMH43XX_Service_DispName="Broadcom 802.11 USB Network Adapter Driver"
BCM435SD_DeviceDesc="Broadcom 802.11ac WDI SDIO Adapter"
BCM4343SD_DeviceDesc="Broadcom 802.11n Wireless SDIO Adapter"
BCMSDH43XX_Service_DispName="Broadcom 802.11 SDIO Network Adapter Driver"
54gAuto="54g - Auto"
54gPerformance="54g - Performance"
80211bOnly="802.11b Only"
AntennaDiversity="Antenna Diversity"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
IBSS54gtmMode="IBSS 54g(tm) Mode"
IBSS54gtmProtectionMode="IBSS 54g(tm) Protection Mode"
IBSSMode="IBSS Mode"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
RadioEnableDisable="Radio Enable/Disable"
Rate="Rate"
RoamingDecision="Roaming Decision"
XPress_Technology="XPress (TM) Technology"
Fast="Fast"
MinimumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
Aux="Aux"
Main="Main"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WMM"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
WZC_Managed_Ethernet="WZC Managed Ethernet"
Legacy="Legacy"
IBSS_Link_Indication="IBSS Link Indication"
Manage_Wireless_Settings="Manage Wireless Settings"
DisableRadioUponWiredConnection="Disable Upon Wired Connect"
SSIDAutoPromote="SSID Autopromote"
IBSSChannelNumber="WZC IBSS Channel Number"
IbssAllowed="IBSS Allowed"
Loose_11h="Loose 11h"
Strict_11h="Strict 11h"
vlan_mode="VLAN Priority Support"
80211bgnAuto="802.11b/g/n Auto"
80211abOnly="802.11a/b Only"
80211abgAuto="802.11a/b/g Auto"
80211abgPerf="802.11a/b/g Performance"
80211abgnAuto="802.11a/b/g/n Auto"
PriorityVLANTag="Priority & VLAN"
PriorityAndVLANDisabled="Priority & VLAN Disabled"
PriorityAndVLANEnabled="Priority & VLAN Enabled"
PriorityEnabled="Priority Enabled"
VLANEnabled="VLAN Enabled"
Lock_Wireless_Settings="Lock Wireless Settings"
Usebestrate="Best Rate"
WakeUpCapabilities="Wake-Up Mode"
NetPattern="Wake Up Frame"
Intolerant="40MHz Intolerant"
All="All"
LossofAP="LossOfLink"
Mixed_Mode="Mixed Mode"
LossNet="WakeUpPkt & LinkLoss"
OBSSCoex="20/40 Coexistance"
BTAMP="BT-AMP"
ListenInterval="Assoc Listen Interval"
D2ListenInterval="D2 Listen Interval"
WFDChannelNumber="WFD Channel Number"
EnableLTR="Enable/Disable LTR"
LTR_ActiveValue="LTR Active value in microseconds"
WakeOnMagicPacket="Wake On Magic Packet"
WakeOnPatternMatch="Wake On Pattern Match"
ARPOffload="ARP Offload"
NSOffload="NS Offload"
WiFiRekeyingOffload="WiFi Rekeying Offload"
PacketCoalescing="Packet Coalescing"
